3.Write an assembly language program for adding two 16-bit data using 8085processor.

LDA 2050

MOV B, A

LDA 2052

ADD B

STA 2053

LDA 2058

MOV B, A

LDA 2059

ADC B

STA 2060

HLT

